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Manse Inspection



Location:

_______________________________________________________
Congregation: 
___________________________________________________
Status:

Occupied / Vacant
Style:


Single Storey / Double Storey
Construction: 
___________________________________________________
Approximate Age: 
________________________
Date Inspected:

________________________
R & D Comm Reps:  
______________________________________________
Congregation Rep: 
_______________________________________________
PRC Comm Rep:
______________________________________________

Other: ____________________________________________________________
Floor Plan:
Supplied / Not Supplied
Original-R & D
Copy-Congregation  Copy-Placements
Copy-Other
_________________________________
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Garden 

Requirement:
A neat practical garden incorporating a self managing design with low maintenance plantings. Trees and shrubs should be dear from the house. Lawn should be well bordered to facilitate efficient mowing. Plants preferably should provide seasonal cut flowers. Garden beds should provide separation and plants should be contained within the beds. Adequate taps or sprinkler system should be provided. A formal vegetable patch is preferred but optional.

Actual: 
Garden condition:
Clean & Tidy / Requires maintenance

Lawn condition:
Clean & Tidy / Requires maintenance

· Low maintenance garden layout.

· Trees & shrubs clear of house.

· Lawn borders constructed for efficient mowing.

· Well formed garden beds.

· Plantings to provide cut flowers.

· Vegetable patch provided.

· Permanent sprinkler system installed, at front / rear side.

· Security conscious external lighting.
Tap Locations: ​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​______________________________________________________________________
Comments:   ________________________________________________________________________

Attention Required:   _________________________________________________________________
Main Entry 

Requirement:
A place of arrival. Externally weatherproof and opening to hallway or similar (i.e.: not directly to Lounge Room or other Living Area).

Actual:
Aspect of door: North / East / South / West

· Letterbox serviceable and secure

· House Number clearly visible

· Main Entry weatherproof (External)

· Main Entry opening to Hallway (or similar)

· Safe passage to doorway - i.e. Floor, handrails if required.

Comments:   _______________________________________________________________________
 Attention Required:   _________________________________________________________________
Entrance Hallway 

Requirement:
Provide seating for 2 to 3 people in privacy (from Living Areas). Provide direct access to Study.

Actual: 

· Seating for 2 to 3 people

· Privacy from Living Areas

· Direct Access to Study

· Electrical Switchboard fitted with Earth Leakage Protection device. 
Floor Covering: 
Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber 

Connection Points: 
Double GPOs: ​​_____
, Single GPOs:_____
, Telephone: _____ , Television ____
Window Coverings:
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar Blinds/Opaque Glass 

Comments: _________________________________________________________________________
Attention Required:  __________________________________________________________________
Study 

Requirement: Preferably not less than 14 square metres floor area. Direct access from Entrance Hall and preferably separate external entry. Provide privacy from the remainder of house. Instantly warmed and cooled, with good natural lighting. Accommodate desk, four drawer filing cabinet, computer and printer.  Space for a photocopier (optional). Fitted with built-in bookshelves not less than 20 linear metres total length and preferably adjustable in height.

Actual:
Floor Area = 
________________ square metres

· Direct access from Entrance Hall

· Separate External Entry

· Private from remainder of house

· Instant heating

· Instant cooling

· Natural lighting


Accommodate: Desk / 4 drawer filing cabinet / Computer & Printer / Photocopier


Bookshelves: 
​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​___________ linear metres total length.

· Shelves height adjustable

Floor Covering:
Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: Double GPOs:_____, Single GPOs:____, Telephone:____, Television: ____

Window Coverings: Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 


Blinds/Opaque Glass

Comments:  ​​​​​​​​​​​​​​​​​​​​​​​​​​_____________________________________________________________________

Attention Required: 
___________________________________________________________

Additional Toilet
Requirement:
Toilet and small basin in separate compartment in close proximity to Study. Readily accessible from  Entrance Hall/Study for visitors. Provide privacy from living areas. Preferably dual flush cistern. Exhaust fan and vanity mirror.

Actual:

· Separate compartment

· Small basin & mirror included

· Privacy from Living Areas

· Dual Flush Cistern

· Exhaust Fan

Accessible from:

· Entry or

· Entrance Hall or

· Study

Floor Covering:
Carpet / Vinyl / Cork Tiles Ceramic Tiles Polished Timber

Connection Points: Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____
Window Coverings: Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 



Blinds/Opaque Glass

Comments:  ​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​​_______________________________________________________________________
Attention Required: 
_________________________________________________________________
Lounge or Living Room 

Requirement:
Preferably not less than 20 square metres floor area. Conveniently located to Main Entry and kitchen. Possible access to Outdoor Living Area.

Actual:
Floor Area = _________________square metres

· Convenient to Main Entry

· Convenient to Kitchen

· Access to Outdoor Living Area

· Combined with Meals Area

· Combined with Dining Room

Floor Covering:
Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________
Dining Room and/or Meals Area 

Requirement:
Preferably not less than 20 square metres floor area. Direct access to Kitchen. May be an extension of the Lounge / Living Room or Kitchen if Meals Area.

Actual:
Floor Area 
​​​​​​​​​​​​​​​​​​​​​​_____________square metres

· Separate Room

·  Extension of Lounge Living Room

· If Meals Area, extension of Kitchen

· Direct Access to Kitchen

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________
Attention Required:__________________________________________________________________
Family Room 

Requirement:
Preferably not less than 15 square metres floor area. Direct access to Kitchen. Access to Garden or Outdoor Living Area.

Actual:
Floor Area = ______________square metres  Direct access to Kitchen
( Access to Garden / Outdoor Living Area

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Kitchen

Requirement: Preferably not less than 10 square metres floor area. Separate from Lounge or Dining / Rooms but may open to Family Room / Meals Area. Access to Laundry and Alternative Rear Entry. Ample built-in cupboards with hard-wearing, sealed bench-top surfaces and splashbacks. Preferably have pantry type food storage cupboard. Dishwasher optional. Spaces to accept refrigerator and separate freezer.

Actual:
Floor Area = 
_______________ square metres
· Separate from Lounge / Dining Areas

· Direct access to Dining Area

· Access to Outdoor Living Area

· Combined with Meals Area

· Open to Family Room

· Access to Laundry

· Access to Rear Entry

· Natural Light

· Pantry type food storage cupboard

· Space for a Refrigerator

· Space for a Freezer

· Space for a Dishwasher

· Dishwasher provided

· Breakfast Bar fitted for stools suitable for snacks

· Ample built-in cupboards with tops of:

Laminate / Marble / Polished Timber / Stainless Steel Ceramic Tiles

Splashbacks: 
Laminate / Ceramic Tiles / Stainless Steel

Sink: 

Number of Bowls _____________________


made from Stainless Steel / Vitreous Enamel

Stove: 

Upright / Wall Oven & Hot plates / Elevated 

powered by: Electricity / Natural Gas / Liquid Petroleum Gas

Ventilation: 
Rangehood / Exhaust Fan

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________
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Laundry 

Requirement:
Equipped with a single or double trough. Sufficient size to accommodate Washing Machine & Tumble Dryer. Preferably storage cupboard and ironing space. Direct access from Passage or similar. Direct access to outside drying area. Clothes line to be fixed and located in a private and secure external area, close to laundry with convenient access.

Actual:
Floor Area = 
_________________ square metres

· Direct access from Passage

· Direct access to outside Drying Area

Number of troughs: ________


· Washing machine bypass

Accommodate:

· Washing Machine

· Tumble Dryer

· Storage Cupboard

· Ironing Space 
Clothes Line:                 Type:  ______________________

   Location: ___________________


· Close access from Laundry

· Private & Secure location

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Passage

Requirement:
To provide access between rooms.

Actual:
Length  __________metres x width __________ metres

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________
Bedroom - Main 

Requirement:
Preferably not less than 14 square metres floor area, including built-in robes or areas for wardrobes Built-in Robes to be not less than 2 metres long x 0.6 metres deep.

Either with en-suite or conveniently located near Bathroom & Toilet facilities.

To accommodate one double bed or two single beds and a dressing table.

Actual:

   Floor Area 
______________ square metres

· En-suite fitted

· Convenient to Bathroom

· Convenient to Toilet

· Built-in- Robes:

long x
deep

· Space for Wardrobes:
long x
deep 
Accommodate:

· One Double Bed, or Two Single Beds

· Dressing Table

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

En-suite (if fitted):
Floor Area:
______________ square metres

· Shower in separate compartment

· Vanity or Storage cabinet with mirror

· Toilet

· Exhaust Fan

· Instant Heat source

· Secure lock on house access door

· Natural light or skylight

· Towel Rails, Total Length:
metres

· Impervious materials on all water contact areas

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Bedroom - Two

Requirement: 
Preferably not less than 14 square metres floor area, including built-in robes or areas for wardrobes Built-in Robes to be not less than 2 metres long x 0.6 metres deep. Conveniently located relative to Main Bedroom, Bathroom & Toilet facilities. To accommodate two single beds, chest of drawers and a study desk.

Actual:
Floor Area = 
____________ square metres

· Convenient to Main Bedroom

· Convenient to Bathroom

· Convenient to Toilet

· Built-in Robes: ____________long x _____________deep

· Space for Wardrobes: __________long x _________deep
Accommodate:

· Two Single Beds or

· One single Bed only.

· and a Chest of Drawers

· and a Study Desk

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Bedroom - Three 

Requirement: Preferably not less than 14 square metres floor area, including built-in robes or areas for wardrobes Built-in Robes to be not less than 2 metres long x 0.6 metres deep. Conveniently located relative to Main Bedroom, Bathroom & Toilet facilities. To accommodate two single beds, chest of drawers and a study desk.

Actual:
Floor Area = 
square metres

· Convenient to Main Bedroom

· Convenient to Bathroom

· Convenient to Toilet

· Built-in Robes: ____________long x _____________deep

· Space for Wardrobes: __________long x _________deep

Accommodate:

· Two Single Beds or

· One Single Bed only.

· and a Chest of Drawers

· and a Study Desk

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Bedroom - Four 

Requirement: Preferably not less than 14 square metres floor area, including built-in robes or areas for wardrobes Built-in Robes to be not less than 2 metres long x 0.6 metres deep. Conveniently located relative to Main Bedroom, Bathroom & Toilet facilities. To accommodate two single beds, chest of drawers and a study desk.

Actual:
Floor Area _______________ square metres

· Convenient to Main Bedroom

· Convenient to Bathroom

· Convenient to Toilet

· Built-in Robes: ____________long x _____________deep

·        Space for Wardrobes: __________long x _________deep

Accommodate:

· Two Single Beds or

· One single Bed only.

· and a Chest of Drawers

· and a Study Desk
Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Bathroom 

Requirement: Impervious material to all water contact splash areas. To be conveniently located to Bedrooms. Full size bath Washbasin (preferably vanity Noe). Storage cabinet with mirror. Towel rails with a minimum total length of 3 metres. Exhaust fan (preferably fan/heater/light unit). Water contact splash areas - bath up to 450mm, basin 300mm.

Actual:
Floor Area ________________square metres
· Convenient to Bedrooms

· Full size bath

· Shower over bath 
Impervious material to water contact splash areas:

· Ceramic Tiles

· Lamnipanel

· Tilux

· Storage cabinet with mirror 

Towel Rail: Total length
 ____________ metres

· Exhaust Fan

· Fan/Heater/Light Unit

· Natural Light/Skylight

· Bathroom includes Toilet

· Bathroom includes Shower

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________
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Page
Shower 

Requirement: Located conveniently to bedrooms. Impervious material to all water contact splash areas - minimum 1.8 metres high. Exhaust fan or fan/heater/light unit

Actual:
Floor Area ________________square metres
· Convenient to Bedrooms

· Separate from Bathroom

· Natural Light/Skylight 

Impervious material to water contact splash areas:

· Ceramic Tiles

· Lamnipanel

· Tilux

· Storage cabinet with mirror 


Towel Rail: Total length __________________ metres

· Exhaust Fan

· Fan/Heater/Light Unit

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Toilet 

Requirement:   Located conveniently to bedrooms.
  Preferably dual flush cistern.
Exhaust fan.

Actual:    Floor Area _______________square metres
· Convenient to Bedrooms

· Separate compartment
i

· Dual flush cistern

· Exhaust Fan

· Natural light/Skylight

· Impervious material to water contact splash areas:

Floor Covering:

Carpet / Vinyl / Cork Tiles / Ceramic Tiles / Polished Timber

Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Window Coverings: 
Curtains/Drapes/Holland Blinds/Venetian Blinds/Vertical Blinds/Cedar 




Blinds/Opaque Glass

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Storage Facilities 

Requirement:
Provide for coats, linen, brooms & vacuum cleaner, suitcases.
Provide a lock up shed to accommodate mower, wheel barrow, garden tools, etc.

Actual:

· Coat Closet
Location: _________________________________________


· Linen Closet
Location: _________________________________________


· Broom Closet
Location: _________________________________________


· Suitcase Storage Location:
_____________________________________
· Storage Shed
Location: 
_____________________________________
· Free Standing Storage Shed:

· Extension of Garage

Construction:
Brick / Timber / Zincalume / Iron Hardiflex

Floor:                        Concrete / Brick / Timber Bare Able to accommodate:

· Mower

· Wheel Barrow

· Garden Tools

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Vehicle Accommodation 

Requirement:
Garage/Carport to accommodate at least one but preferably two cars. May be free standing or an extension of the house. Preferably undercover access between house and garage. Garage to accommodate work bench with power outlet.

Actual:

Double Garage/Single Garage & Carport/Single Garage/Carport only

· Free Standing

· Extension of House

· Undercover Access

· Accommodate a Work Bench

Construction: 
Brick / Timber / Zincalume Iron Hardiflex

Floor:


Concrete / Brick Timber / Crushed Rock / Bare

Roof:


Tile / Zincalume Galvanized Iron

Location Relative to House: _____________________________________________


Connection Points: 
Double GPOs: ____
 Single GPOs: ____ Telephone:____, Television: ____

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Exterior 

Paintwork 

Requirement:
To be in good condition, free from flaking, peeling, cracking or other surface defects and imperfections.

Actual: 
Item




Condition


__________________________    _________________________________________


__________________________    _________________________________________


__________________________    _________________________________________


__________________________    _________________________________________



_________________

_____________________


Attention Required:__________________________________________________________________

Stormwater

Requirement:
Spouting and downpipes to be in good condition with no evidence of corrosion, defective joins or water leaks. Fall of spouting to be towards outlets into downpipes. Access points for clearing underground stormwater drains desirable.

Actual: 
Item




Condition


__________________________    _________________________________________


__________________________    _________________________________________


__________________________    _________________________________________


__________________________    _________________________________________



_________________

_____________________


Attention Required:__________________________________________________________________

Roof

Requirement:
To be of weatherproof material and have adequate 'fall' on all aspects to discharge all rain water into stormwater spoutings. All roof surface/vertical projection junctions to be sealed to prevent ingress of water.

Actual:
Material:
Terracotta Tiles Cement Tiles / Slate Tiles / Galv Iron Zincalume 

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Sun Blinds 

Requirement:
Desirable where heat penetration from excessive summer sun is a problem. 
Actual:
Not fitted to any window / Fitted to the following windows:   _________________________________________________________________________________________

_________________________________________________________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Insect Screens 

Requirement:
To be fitted to all windows and external doors on dwelling. External 'screen' doors to be lockable 


security doors

Actual:

Fitted to all windows / Not fitted to any windows.

Fitted to:
______________________________________________________________window(s).

Screen doors to:  ____________________________________________________________________

Security doors to:  ___________________________________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Paving 

Requirement:
Hard surfaces should be provided for Garage/Carport tracks, Clothes Hoist track, and, front entry 


track. May be Concrete, Crushed Rock, Paving Stones, Bricks, Cement Slabs or similar.
Actual:
Item




Condition


__________________________    _________________________________________

__________________________    _________________________________________


__________________________    _________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________

Fences 

Requirement:
Appropriate to provide privacy and security.
Actual:
Material



Estimated Life Remaining

__________________________    _________________________________________

__________________________    _________________________________________


__________________________    _________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Attention Required:__________________________________________________________________
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Basic Equipment

Heating / Cooling 

Requirement:
Heating to be in Lounge, Dining Room, Family Room and Study. Cooling in rooms where necessary due to the aspect of the dwelling.

Actual:

· Ducted System: Heating Only / Cooling Only / Heating & Cooling 
Outlets in: _______________________________________________________

· Individual Room Heating 
Outlets in: _______________________________________________________

· Individual Room Cooling 
Outlets in: _______________________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Hot Water System 

Requirement:
Mains pressure preferred. Capable of supplying normal household requirements.

Actual:

Supply Pressure: 

Mains Storage

Fuel:



Natural Gas / LP Gas / Electric Slow Combustion / Solar Location: 


Internal / External

Capacity: 


_______________ Litres
· fitted Hot Water Temperature Limiting Valve
Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Insulation 

Requirement:
Essential in ceilings. Desirable in walls.
Actual:

· Installed in ceilings 
Type:
_________________________________________
· Installed in walls
Type:  _________________________________________

Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Smoke Detectors 

Requirement:
Minimum of 2 essential. Mains supply preferred. Battery only acceptable if mains type can't be installed.

Actual:
Number installed:_._ Power Supply type: Locations: 
 Mains / Battery
Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________

Television Antenna 

Requirement:
Sufficient to provide good quality reception to all connection points in dwelling.
Actual:


Reception Quality:
 ______________________________________________
Comments: ​​​​​​​​​​​​​​​​________________________________________________________________________
Additional Comments 

________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________

Summary 

________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________
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